,Circuit Watts##ELECTRICAL_WATTAGE##WATTS,Sap Code##OTHER##,Rating##OTHER##,Photometric Web File##OTHER##,Mass##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Emergency luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS
GLACIER II LED 5500 HFIX E3 GL PR L830,56,96221137,56,GLACIER II LED 5500 HFIX GL PR L830.IES,7.1,5705,3000,102,94
GLACIER II LED 5500 HFIX E3 PC PR L830,56,96221136,56,GLACIER II LED 5500 HFIX PC PR L830.IES,5.3,5602,3000,100,93
GLACIER II LED2 3000 HFIX E3 GL PR L830,26.5,96629052,26.5,GLACIER II LED2 3000 HFIX EC GL PR 830.IES,7.1,2900,3000,109,105
GLACIER II LED2 3000 HFIX E3 PC PR L830,26.5,96629051,26.5,GLACIER II LED2 3000 HFIX EC PC PR 830.IES,5.3,2900,3000,109,105
GLACIER II LED2 3500 HFIX E3 GL PR L840,26.5,96629055,26.5,GLACIER II LED2 3500 HFIX EC GL PR 840.IES,7.1,3050,4000,115,105
GLACIER II LED2 3500 HFIX E3 PC PR L840,26.5,96629054,26.5,GLACIER II LED2 3500 HFIX EC PC PR 840.IES,5.3,3000,4000,113,105
GLACIER II LED2 6000 HFIX E3 GL PR L840,45.5,96629061,45.5,GLACIER II LED2 6000 HFIX EC GL PR 840.IES,7.1,5400,4000,119,105
GLACIER II LED2 6000 HFIX E3 PC PR L840,45.5,96629060,45.5,GLACIER II LED2 6000 HFIX EC PC PR 840.IES,5.3,5350,4000,118,105
,,,,,,,,,
,,,,,,,,,
