,Circuit Watts##ELECTRICAL_WATTAGE##WATTS,Power Factor##OTHER##,Sap Code##OTHER##,Rating##OTHER##,Photometric Web File##OTHER##,Mass##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Emergency luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS
GLACIER II LED 3000 HFIX E3 AL L830,36,0.95,96221131,36,GLACIER II LED 3000 HFIX AL L830.IES,5.1,2710,3000,75,80
GLACIER II LED 3500 HFIX E3 AL L840,36,0.95,96221135,36,GLACIER II LED 3500 HFIX AL L840.IES,5.1,2872,4000,80,80
GLACIER II LED 5500 HFIX E3 AL L830,56,0.95,96221139,56,GLACIER II LED 5500 HFIX AL L830.IES,5.1,4655,3000,83,80
GLACIER II LED 6000 HFIX E3 AL L840,56,0.95,96221143,56,GLACIER II LED 6000 HFIX AL L840.IES,5.1,4934,4000,88,80
