,Circuit Watts##ELECTRICAL_WATTAGE##WATTS,Sap Code##OTHER##,Rating##OTHER##,Photometric Web File##OTHER##,Mass##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT
GLACIER II LED 5500 HFIX GL OP L830,56,96221106,56,GLACIER II LED 5500 HFIX GL OP L830.IES,6.5,5721,3000,102
GLACIER II LED 5500 HFIX GL PR L830,56,96221105,56,GLACIER II LED 5500 HFIX GL PR L830.IES,6.8,5705,3000,102
GLACIER II LED 5500 HFIX PC PR L830,56,96221104,56,GLACIER II LED 5500 HFIX PC PR L830.IES,5,5602,3000,100
GLACIER II LED2 3000 HFIX EC GL OP 830,26.5,96629031,26.5,GLACIER II LED2 3000 HFIX EC GL OP 830.IES,6.5,2950,3000,111
GLACIER II LED2 3000 HFIX EC GL PR 830,26.5,96629033,26.5,GLACIER II LED2 3000 HFIX EC GL PR 830.IES,6.8,2900,3000,109
GLACIER II LED2 3000 HFIX EC PC PR 830,26.5,96629035,26.5,GLACIER II LED2 3000 HFIX EC PC PR 830.IES,5,2900,3000,109
GLACIER II LED2 3500 HFIX EC GL OP 840,26.5,96629032,26.5,GLACIER II LED2 3500 HFIX EC GL OP 840.IES,6.5,3050,4000,115
GLACIER II LED2 3500 HFIX EC GL PR 840,26.5,96629034,26.5,GLACIER II LED2 3500 HFIX EC GL PR 840.IES,6.8,3050,4000,115
GLACIER II LED2 3500 HFIX EC PC PR 840,26.5,96629036,26.5,GLACIER II LED2 3500 HFIX EC PC PR 840.IES,5,3000,4000,113
GLACIER II LED2 6000 HFIX EC GL OP 840,45.5,96629040,45.5,GLACIER II LED2 6000 HFIX EC GL OP 840.IES,6.5,5500,4000,121
GLACIER II LED2 6000 HFIX EC GL PR 840,45.5,96629042,45.5,GLACIER II LED2 6000 HFIX EC GL PR 840.IES,6.8,5400,4000,119
GLACIER II LED2 6000 HFIX EC PC PR 840,45.5,96629044,45.5,GLACIER II LED2 6000 HFIX EC PC PR 840.IES,5,5350,4000,118
